[INSTALL_SEQUENCE]
//INSTALL_1="UNINSTALL_PROGRAM"
INSTALL_2="COMMAND_SYSTEM_ID"

[UNINSTALL_PROGRAM]
UNINSTALL="Alcor Micro Card Reader Driver"

[INSTALL_MSI_PROGRAM]

[COMMAND]
COMMAND_1="install.cmd"

[COMMAND_INSTALL]

[SYSTEM_ID]
SYSTEM_ID_1="8477"
SYSTEM_ID_2="8478"
SYSTEM_ID_3="8479"

[COMMAND_SYSTEM_ID]
//%SYSID% defines command sequence for specific system ID
SYSTEM_ID_1="COMMAND_1"
SYSTEM_ID_2="COMMAND_1"
SYSTEM_ID_3="COMMAND_1"

[RETURN_CODE]
RETURN_CODE_32="INSTALL_32"
RETURN_CODE_64="INSTALL_64"

[RETURN_CODE_TRANSLATION]
//%1 defines specific return code from execution command return by RETURN_CODE
//Setup.exe returns translated return code.
//HPSA Supported return codes are: 0="Success", 259="Failure", 1602="Cancel", 3010="Success Reboot Required"
//Intel returns 14 as "Success Reboot Required"
14="3010"
