; Copyright (c) 2009-2014 Intel Corporation  
; **********************************************************************************************  
; **********************************************************************************************  
; **    Filename:  iaStorA.inf  
; **    Revision:  DRIVER_INFO 
; **    Abstract:  Windows* INF File for AHCI Intel(R) Rapid Storage Technology Enterprise Driver  
; **               Installs: RSTe AHCI RAID Controller Miniport (without RST Filter Driver) 
; **               Only for Windows 8 releases 
; **********************************************************************************************  
; 
[Version]  
Signature="$Windows NT$"  
Provider=%INTEL%  
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}  
Class=SCSIAdapter  
CatalogFile=iaStorA.cat  
DriverVer=07/14/2015,4.3.1.1152
; 
[PackageInfo]  
Name=AHCI  
; 
[SourceDisksNames]  
1 = %DiskId1%,,,""  
; 
[DestinationDirs]  
DefaultDestDir = 12  
; 
[ControlFlags]  
ExcludeFromSelect = *  
; 
[Manufacturer]  
%INTEL% = INTEL, NTamd64.6.2, NTamd64.6.3, NTamd64.10.0   
[iaStorA_Service_Inst]  
ServiceType    = %SERVICE_KERNEL_DRIVER%  
StartType      = %SERVICE_BOOT_START%  
ErrorControl   = %SERVICE_ERROR_NORMAL%  
ServiceBinary  = %12%\iaStorA.sys  
LoadOrderGroup = SCSI miniport  
AddReg         = pnpsafe_pci_addreg  
; 
[iaStorA_EventLog_Inst]  
AddReg = iaStorA_EventLog_AddReg  
; 
[iaStorA_EventLog_AddReg]  
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorA.sys" 
HKR,,TypesSupported,%REG_TYPE_DWORD%,7  
;
;********************************************************  
;*  
;* 64-BIT X86 ARCHITECTURE  
;*  
;* This section specifies the 64-bit architecture specific INF file entries  
;* required to install a driver as a 64-bit compatible driver.  
;*  
;******************************************************************************  
[SourceDisksFiles.amd64]   
iaStorA.sys = 1,,,   
; 
[INTEL.NTamd64.10.0] 
;windows_10_64-bit and later 
%PCI\VEN_8086&DEV_2826&SUBSYS_047D1014.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_047D1014
%PCI\VEN_8086&DEV_2826&SUBSYS_04811014.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_04811014
%PCI\VEN_8086&DEV_2826&SUBSYS_04851014.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_04851014
%PCI\VEN_8086&DEV_2826&SUBSYS_11B61734.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_11B61734
%PCI\VEN_8086&DEV_2826&SUBSYS_201019E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201019E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201219E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201219E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201319E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201319E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201519E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201519E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201619E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201619E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201B19E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201B19E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201D19E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201D19E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201F19E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201F19E5
%PCI\VEN_8086&DEV_2826&SUBSYS_28228086.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_28228086
%PCI\VEN_8086&DEV_2826&SUBSYS_306E1054.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_306E1054
%PCI\VEN_8086&DEV_2826&SUBSYS_72708086.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_72708086
%PCI\VEN_8086&DEV_2826&CC_0104.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&CC_0104
;  
[INTEL.NTamd64.6.3] 
;windows_8.1_64-bit 
%PCI\VEN_8086&DEV_2826&SUBSYS_047D1014.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_047D1014
%PCI\VEN_8086&DEV_2826&SUBSYS_04811014.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_04811014
%PCI\VEN_8086&DEV_2826&SUBSYS_04851014.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_04851014
%PCI\VEN_8086&DEV_2826&SUBSYS_11B61734.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_11B61734
%PCI\VEN_8086&DEV_2826&SUBSYS_201019E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201019E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201219E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201219E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201319E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201319E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201519E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201519E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201619E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201619E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201B19E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201B19E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201D19E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201D19E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201F19E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201F19E5
%PCI\VEN_8086&DEV_2826&SUBSYS_28228086.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_28228086
%PCI\VEN_8086&DEV_2826&SUBSYS_306E1054.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_306E1054
%PCI\VEN_8086&DEV_2826&SUBSYS_72708086.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_72708086
%PCI\VEN_8086&DEV_2826&CC_0104.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&CC_0104
;  
[INTEL.ntamd64.6.2] 
;windows_8_64-bit 
%PCI\VEN_8086&DEV_2826&SUBSYS_047D1014.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_047D1014
%PCI\VEN_8086&DEV_2826&SUBSYS_04811014.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_04811014
%PCI\VEN_8086&DEV_2826&SUBSYS_04851014.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_04851014
%PCI\VEN_8086&DEV_2826&SUBSYS_11B61734.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_11B61734
%PCI\VEN_8086&DEV_2826&SUBSYS_201019E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201019E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201219E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201219E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201319E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201319E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201519E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201519E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201619E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201619E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201B19E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201B19E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201D19E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201D19E5
%PCI\VEN_8086&DEV_2826&SUBSYS_201F19E5.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_201F19E5
%PCI\VEN_8086&DEV_2826&SUBSYS_28228086.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_28228086
%PCI\VEN_8086&DEV_2826&SUBSYS_306E1054.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_306E1054
%PCI\VEN_8086&DEV_2826&SUBSYS_72708086.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&SUBSYS_72708086
%PCI\VEN_8086&DEV_2826&CC_0104.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_2826&CC_0104
;  
[iaStorA_inst.ntamd64] 
CopyFiles=@iaStorA.sys  
FeatureScore=0x80
; 
[iaStorA_inst.ntamd64.HW]  
AddReg = msi_addreg  
AddReg = storport_addreg 
AddReg = sgpio_addreg 
; 
[iaStorA_inst.ntamd64.Services]  
AddService = iaStorA, %SPSVCINST_ASSOCSERVICE%, iaStorA_Service_Inst, iaStorA_EventLog_Inst  
; 
[pnpsafe_pci_addreg] 
; Use raw values for BusType, not a DEFINE, ChkInf fails on hex alpha chars  
; BusType_ATA == 0x3, BusTypeATA, BusType_RAID == 0x8, BusType_SATA == 0xb  
HKR, Parameters\PnpInterface,  5,                           %REG_TYPE_DWORD%,  0x00000001  
HKR, Parameters,               BusType,                     %REG_TYPE_DWORD%,  0x00000008 
; Tell Storport in Win7/Srv08R2(KB982018) that driver can report 4K sector size (not needed in Win8) 
HKR, Parameters\Device,        EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001 
; 
[Strings]  
; Localizable Strings  
; 
diskId1 = "RSTe Installation Disk"  
;server 
PCI\VEN_8086&DEV_2826&SUBSYS_047D1014.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_04811014.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_04851014.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_11B61734.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_201019E5.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_201219E5.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_201319E5.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_201519E5.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_201619E5.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_201B19E5.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_201D19E5.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_201F19E5.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_28228086.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_306E1054.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&SUBSYS_72708086.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller"
PCI\VEN_8086&DEV_2826&CC_0104.DeviceDesc = "Intel(R) C600+/C220+ series chipset SATA RAID Controller" 
; 
INTEL = "Intel Corporation"  
; 
; Non-Localizable Strings  
; 
SPSVCINST_ASSOCSERVICE = 0x00000002  
REG_MULTI_SZ           = 0x00010000  
REG_EXPAND_SZ          = 0x00020000  
REG_TYPE_DWORD         = 0x00010001  
SERVICE_KERNEL_DRIVER  = 1  
SERVICE_BOOT_START     = 0  
SERVICE_ERROR_NORMAL   = 1 
; 
; MSI enables.  
; 
[msi_addreg]   
HKR, Interrupt Management, 0x00000010   
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010   
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_TYPE_DWORD%,   1   
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_TYPE_DWORD%,   1  
; 
[storport_addreg] 
;;; Enables/Disables Idle Power Management for StorPort 
HKR, "StorPort", "EnableIdlePowerManagement", %REG_TYPE_DWORD%, 0x00000001 
; 
[sgpio_addreg] 
;;; Enable/disable SGPIO support 
HKLM, System\CurrentControlSet\Services\iaStorA\Parameters\Device, LED_Supported, %REG_TYPE_DWORD%, 0x00000001 
