;-------------------------------------------------------------------------------
;
; Motorola USB Networking Driver (motousbnet.inf)
;
; Copyright (c) Motorola Mobility Inc
;
;-------------------------------------------------------------------------------

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Motorola%
DriverVer   = 03/01/2013, 2.7.0.0
CatalogFile = motousbnet.cat

[ControlFlags]
ExcludeFromSelect=*

[DestinationDirs]
Motousbnet.CopyFiles = 12

[Motousbnet.CopyFiles]
Motousbnet.sys,,,2
motfilt.sys,,,2
motswch.sys,,,2

[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles]
Motousbnet.sys = 1,,
motswch.sys = 1,,
motfilt.sys = 1,,
wdfcoinstaller01009.dll = 1,,

; Models -----------------------------------------------------------------------

[Manufacturer]
%Motorola% = Motorola,NTamd64

[Motorola]

; q xs
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E72&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E73&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E74&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E75&MI_06

; test
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_41EE&MI_02

; q sm
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E50&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E51&MI_01

; q dva
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E34&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E35&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E37&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E38&MI_02

; i
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7101
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7102&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7103&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7104&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7105&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7106&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7109&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_710A&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_710D&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_710E&MI_01

; ics qc d
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E28&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E29&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E2A&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E2B&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E2C
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E2D&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E32&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E33&MI_01

; ics o4
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4355&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4356&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435D&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435E&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4361&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4362&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4363&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4364&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4353&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4354&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435B&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435C&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_433C&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_433D&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_433E&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_433F&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4305&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4306&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4307&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4308&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4357&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4358&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435F&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4360&MI_01

; g2
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41C6&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41C7&MI_00

; p qc
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DF2
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DF3&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DF4&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DF5&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DFE&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DFF&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2E01&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2E02&MI_00
; o4
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4310&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4311&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_433A&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_433B&MI_00

; o4-1
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4312
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4313&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4314&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4315&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_431F&MI_04
; o4-2
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4330&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4331&MI_02

; h nV
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70AA&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70AB&MI_02
; et
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7093&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7094&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7095&MI_0A
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7096&MI_0A
;ev 
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70B0&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70B1&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70B2&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70B3&MI_08
; t o4
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_42F2
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_42F3&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_42F4&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_42F5&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_4301&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_4302&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_4303&MI_0A
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_4304&MI_0A
; s o4
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_42D2
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_42D3&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_42D4&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_42D5&MI_02
; d nV
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70C2
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70C3&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70C4&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70C5&MI_02

; e
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70A2&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70A3

; g,o3
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41D5&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41E6&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41E7&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41E8&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41E9&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41EA&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41ED&MI_02
; c
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DD0&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DD3&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DD8&MI_01
; o/e
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7080&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7081&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7082&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7083
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_708A&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_708B&MI_02
; s
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_4283&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_4284&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_428A
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_428B&MI_00
; d2
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42A1&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42A2&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42A8
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42A9&MI_00
; dp
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42B1&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42B2&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42B8
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42B9&MI_00
; v2
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42C1&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42C2&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42C8
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42C9&MI_00
; calgary
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D7A&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D7B&MI_02

; Morrison/Motus/Zepplin
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D68&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D69&MI_01
;Beihai
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_4272

;Calgary
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D71&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D74&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D79&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D7A&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D7B&MI_02

;Sholes CDMA
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_41E2&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_41E3&MI_02

%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2C69&MI_03
;morrison
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D61&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D63&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D64&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D65&MI_01

%Motousbnet.DeviceDesc% = Motousbnet.ndi2, USB\VID_22b8&PID_4192
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6027
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424&MI_03
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6425&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6425&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6425&MI_03
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6425&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6427&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6427&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6427&MI_03
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6427&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_41D4
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_41D8&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_41DA&MI_02


[Motorola.NTamd64]

; q xs
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E72&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E73&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E74&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E75&MI_06

; test
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_41EE&MI_02

; q sm
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E50&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E51&MI_01

; q dva
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E34&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E35&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E37&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E38&MI_02

; i
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7101
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7102&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7103&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7104&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7105&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7106&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_7109&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_710A&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_710D&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_710E&MI_01

; ics qc d
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E28&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E29&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E2A&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E2B&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E2C
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E2D&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E32&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_2E33&MI_01

; ics o4
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4355&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4356&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435D&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435E&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4361&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4362&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4363&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4364&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4353&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4354&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435B&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435C&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_433C&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_433D&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_433E&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_433F&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4305&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4306&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4307&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4308&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4357&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4358&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_435F&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_4360&MI_01

; g2
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41C6&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41C7&MI_00

; p qc
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DF2
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DF3&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DF4&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DF5&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DFE&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DFF&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2E01&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2E02&MI_00
; o4
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4310&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4311&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_433A&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_433B&MI_00

; o4-1
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4312
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4313&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4314&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4315&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_431F&MI_04
; o4-2
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4330&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_4331&MI_02

; h nV
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70AA&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70AB&MI_02
; et
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7093&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7094&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7095&MI_0A
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7096&MI_0A
;ev 
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70B0&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70B1&MI_06
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70B2&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70B3&MI_08
; t o4
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_42F2
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_42F3&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_42F4&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_42F5&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_4301&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_4302&MI_08
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_4303&MI_0A
%Motousbnet.DeviceDesc% = Motousbnet.ndi4, USB\VID_22b8&PID_4304&MI_0A
; s o4
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_42D2
%Motousbnet.DeviceDesc% = Motousbnet.ndi5, USB\VID_22b8&PID_42D3&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_42D4&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_42D5&MI_02
; d nV
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70C2
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70C3&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70C4&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70C5&MI_02

; e
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70A2&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_70A3

; g,o3
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41D5&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41E6&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41E7&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41E8&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41E9&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41EA&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_41ED&MI_02
; c
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DD0&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DD3&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2DD8&MI_01
; o/e
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7080&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7081&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7082&MI_00
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_7083
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_708A&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_708B&MI_02
; s
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_4283&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_4284&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_428A
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_428B&MI_00
; d2
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42A1&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42A2&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42A8
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42A9&MI_00
; dp
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42B1&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42B2&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42B8
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42B9&MI_00
; v2
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42C1&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42C2&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42C8
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22B8&PID_42C9&MI_00
; calgary
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D7A&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D7B&MI_02

; Morrison/Motus/Zepplin
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D68&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D69&MI_01
;Beihai
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_4272

;Calgary
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D71&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D74&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D79&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D7A&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D7B&MI_02

;Sholes CDMA
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_41E2&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_41E3&MI_02

%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2C69&MI_03
;morrison
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D61&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D63&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D64&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi0, USB\VID_22b8&PID_2D65&MI_01

%Motousbnet.DeviceDesc% = Motousbnet.ndi2, USB\VID_22b8&PID_4192
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6027
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424&MI_03
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6424&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6425&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6425&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6425&MI_03
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6425&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6427&MI_01
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6427&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6427&MI_03
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_6427&MI_04
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_41D4
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_41D8&MI_02
%Motousbnet.DeviceDesc% = Motousbnet.ndi1, USB\VID_22b8&PID_41DA&MI_02

; Model sections ---------------------------------------------------------------

[Motousbnet.ndi0]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 15 ; if you specify NCF_PHYSICAL, you must specify bustype
AddReg          = Motousbnet.Reg, ParamsPromiscuous, Motousbnet.ndi.AddReg
CopyFiles       = Motousbnet.CopyFiles

[Motousbnet.ndi0.HW]
AddReg          = Motousbnet.ndi.AddReg, Motousbnet_HW_Cfg0

[Motousbnet.ndi1]
Characteristics = 0x84 ; NCF_PHYSICAL
BusType         = 15 ; if you specify NCF_PHYSICAL, you must specify bustype
AddReg          = Motousbnet.Reg, ParamsPromiscuous, Motousbnet.ndi.AddReg
CopyFiles       = Motousbnet.CopyFiles

[Motousbnet.ndi1.HW]
AddReg          = Motousbnet.ndi.AddReg, Motousbnet_HW_Cfg1

[Motousbnet.ndi2]
Characteristics = 0x84 ; NCF_PHYSICAL
BusType         = 15 ; if you specify NCF_PHYSICAL, you must specify bustype
AddReg          = Motousbnet.Reg, ParamsPromiscuous, Motousbnet.ndi.AddReg
CopyFiles       = Motousbnet.CopyFiles

[Motousbnet.ndi2.HW]
AddReg          = Motousbnet.ndi.AddReg, Motousbnet_HW_Cfg2

[Motousbnet.ndi4]
Characteristics = 0x84 ; NCF_PHYSICAL  + NCF_HAS_UI
BusType         = 15 ; if you specify NCF_PHYSICAL, you must specify bustype
AddReg          = Motousbnet.Reg, ParamsPromiscuous, Motousbnet.ndi.AddReg
CopyFiles       = Motousbnet.CopyFiles

[Motousbnet.ndi4.HW]
AddReg          = Motousbnet.ndi.AddReg, Motousbnet_HW_Cfg4

[Motousbnet.ndi5]
Characteristics = 0x84 ; NCF_PHYSICAL  + NCF_HAS_UI
BusType         = 15 ; if you specify NCF_PHYSICAL, you must specify bustype
AddReg          = Motousbnet.Reg, ParamsPromiscuous, Motousbnet.ndi.AddReg
CopyFiles       = Motousbnet.CopyFiles

[Motousbnet.ndi5.HW]
AddReg          = Motousbnet.ndi.AddReg, Motousbnet_HW_Cfg5

; Services ---------------------------------------------------------------------

[Motousbnet.ndi0.Services]
AddService      = Motousbnet, 2, Motousbnet.Service, Motousbnet.EventLog
AddService      = MotoSwitchService,,MotoSwitch_Service_Inst
AddService      = BTCFilterService,,BTC_Filter_Service_Inst

[Motousbnet.ndi1.Services]
AddService      = Motousbnet, 2, Motousbnet.Service, Motousbnet.EventLog
AddService      = MotoSwitchService,,MotoSwitch_Service_Inst
AddService      = BTCFilterService,,BTC_Filter_Service_Inst

[Motousbnet.ndi2.Services]
AddService      = Motousbnet, 2, Motousbnet.Service, Motousbnet.EventLog
AddService      = MotoSwitchService,,MotoSwitch_Service_Inst
AddService      = BTCFilterService,,BTC_Filter_Service_Inst

[Motousbnet.ndi4.Services]
AddService      = Motousbnet, 2, Motousbnet.Service, Motousbnet.EventLog
AddService      = MotoSwitchService,,MotoSwitch_Service_Inst
AddService      = BTCFilterService,,BTC_Filter_Service_Inst

[Motousbnet.ndi5.Services]
AddService      = Motousbnet, 2, Motousbnet.Service, Motousbnet.EventLog
AddService      = MotoSwitchService,,MotoSwitch_Service_Inst
AddService      = BTCFilterService,,BTC_Filter_Service_Inst

[Motousbnet.ndi.AddReg]
HKR,,"UpperFilters",0x00010000,MotoSwitchService,BTCFilterService

; Device Parameters Entries ----------------------------------------------------

[Motousbnet_HW_Cfg0]
HKR, , MotConfigFlag, 0x00010001, 0

[Motousbnet_HW_Cfg1]
HKR, , MotConfigFlag, 0x00010001, 1

[Motousbnet_HW_Cfg2]
HKR, , MotConfigFlag, 0x00010001, 2

[Motousbnet_HW_Cfg4]
HKR, , MotConfigFlag, 0x00010001, 4

[Motousbnet_HW_Cfg5]
HKR, , MotConfigFlag, 0x00010001, 5

; Service installation ---------------------------------------------------------

[MotoSwitch_Service_Inst]
DisplayName     = "MotoSwitch Service"
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 0 ;%SERVICE_ERROR_IGNORE%
ServiceBinary   = %12%\motswch.sys
LoadOrderGroup  = extended base

[BTC_Filter_Service_Inst]
DisplayName     = "USB Networking Driver Filter Service"
ServiceType     = 1    ; SERVICE_KERNEL_DRIVER
StartType       = 3    ; SERVICE_AUTO_START
ErrorControl    = 0    ; NORMAL
ServiceBinary   = %12%\motfilt.sys
LoadOrderGroup  = PNP Filter

[Motousbnet.Service]
DisplayName     = %Motousbnet.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Motousbnet.sys
LoadOrderGroup  = NDIS
AddReg          = TextModeFlags.Reg

[Motousbnet.EventLog]
AddReg = Motousbnet.AddEventLog.Reg

[Motousbnet.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[TextModeFlags.Reg]
HKR, , TextModeFlags,    0x00010001, 0x0001

; Miniport common --------------------------------------------------------------

[Motousbnet.Reg]
HKR,    ,                         BusNumber,           0, "0"
HKR, Ndi,                         Service,             0, "Motousbnet"
HKR, Ndi\Interfaces,              UpperRange,          0, "ndis5"
HKR, Ndi\Interfaces,              LowerRange,          0, "ethernet"

[ParamsPromiscuous]
;
;    Should the physical NIC be set to Promiscuous mode
;
HKR, Ndi\Params\Promiscuous,     ParamDesc, , %Promiscuous%
HKR, Ndi\Params\Promiscuous,     Default,  ,"0"
HKR, Ndi\Params\Promiscuous,     type, ,      enum
HKR, Ndi\Params\Promiscuous\enum,"1",  ,     %Promiscuous_Enable%
HKR, Ndi\Params\Promiscuous\enum,"0",  ,     %Promiscuous_Disable%

; Coinstaller installation -----------------------------------------------------

[DestinationDirs]
Motousbnet_CoInstaller_CopyFiles = 11

[Motousbnet.ndi0.CoInstallers]
AddReg    = Motousbnet_CoInstaller_AddReg
CopyFiles = Motousbnet_CoInstaller_CopyFiles

[Motousbnet.ndi1.CoInstallers]
AddReg    = Motousbnet_CoInstaller_AddReg
CopyFiles = Motousbnet_CoInstaller_CopyFiles

[Motousbnet.ndi2.CoInstallers]
AddReg    = Motousbnet_CoInstaller_AddReg
CopyFiles = Motousbnet_CoInstaller_CopyFiles

[Motousbnet.ndi4.CoInstallers]
AddReg    = Motousbnet_CoInstaller_AddReg
CopyFiles = Motousbnet_CoInstaller_CopyFiles

[Motousbnet.ndi5.CoInstallers]
AddReg    = Motousbnet_CoInstaller_AddReg
CopyFiles = Motousbnet_CoInstaller_CopyFiles

[Motousbnet_CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "wdfcoinstaller01009.dll,WdfCoInstaller"

[Motousbnet_CoInstaller_CopyFiles]
wdfcoinstaller01009.dll

[SourceDisksFiles]
wdfcoinstaller01007.dll=1 ; make sure the number matches with SourceDisksNames

[Motousbnet.ndi0.Wdf]
KmdfService = Motousbnet, Motousbnet_wdfsect
KmdfService = BTCFilterService, BTCFilterService_wdfsect

[Motousbnet.ndi1.Wdf]
KmdfService = Motousbnet, Motousbnet_wdfsect
KmdfService = BTCFilterService, BTCFilterService_wdfsect

[Motousbnet.ndi2.Wdf]
KmdfService = Motousbnet, Motousbnet_wdfsect
KmdfService = BTCFilterService, BTCFilterService_wdfsect

[Motousbnet.ndi4.Wdf]
KmdfService = Motousbnet, Motousbnet_wdfsect
KmdfService = BTCFilterService, BTCFilterService_wdfsect

[Motousbnet.ndi5.Wdf]
KmdfService = Motousbnet, Motousbnet_wdfsect
KmdfService = BTCFilterService, BTCFilterService_wdfsect

[Motousbnet_wdfsect]
KmdfLibraryVersion = 1.9

[BTCFilterService_wdfsect]
KmdfLibraryVersion = 1.9

; Strings ----------------------------------------------------------------------

[Strings]
Motorola                    = "Motorola"
Motousbnet.DeviceDesc       = "Motorola USB Networking Driver"
Motousbnet.Service.DispName = "Motorola USB Networking Driver Service"
DiskId1                     = "Motorola USB Networking Driver Disk #1"
Promiscuous                 = "Set the physical NIC to promiscuous mode"
Promiscuous_Disable         = "Disable"
Promiscuous_Enable          = "Enable"
