;
; Android WinUsb driver installation.
;
[Version]
Signature           = "$Windows NT$"
Class               = AndroidUsbDeviceClass
ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider            = %ProviderName%
; month/day/year
DriverVer           = 06/20/2014,7.0.0000.00001
CatalogFile.NTx86   = androidwinusb86.cat
CatalogFile.NTamd64 = androidwinusba64.cat

[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1


[Manufacturer]
%ProviderName% = Google, NTx86, NTamd64


[Google.NTx86]
;;;;;;;;;;;;;;;;;;;;;;CMCC USB history NTx86;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
;MT65xx meta mode
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005&MI_01
;CMCC ADB Interface
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74A4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_200F
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0C03&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05c6&PID_9025&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0005
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0005&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D00D
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7495&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74EC&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7509&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05c6&PID_0001&MI_01   
;;;;;;;;;;;;;;;;;;;;;;CMCC USB history end NTx86;;;;;;;;;;;;;;;;;;;;;;;; 

;;;;;;;;;;;;;;;;;;;;;;CMCC USB Factory NTx86;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
; Shellw rndis,diag,adb
%CompositeAdbInterface% = USB_Install, USB\VID_05C6&PID_902D&MI_03
;;;;;;;;;;;;;;;;;;;;;;CMCC USB Factory end NTx86;;;;;;;;;;;;;;;;;;;;;;;;;;;; 

;;;;;;;;;;;;;;;;;;;;;;CMCC USB generic NTx86;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
;generic mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7435&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2009&MI_01
;generic mass_storage,adb,acm
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74ED&MI_01
;generic adb,diag,modem,nmea
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7501&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_200D&MI_00
;generic adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7513&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2000&MI_00
;generic mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F8&MI_01
;generic ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2005&MI_01
;generic rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7500&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2003&MI_02
;generic bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750E&MI_01
;generic mtp,adb,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74EE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_200C&MI_01
;generic mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7718&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2008&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2006&MI_02
;;;;;;;;;;;;;;;;;;;;;;CMCC USB generic end NTx86;;;;;;;;;;;;;;;;;;;;;;;;; 
      
;;;;;;;;;;;;;;;;;;;;;;CMCC USB Project NTx86;;;;;;;;;;;;;;;;;;;;;;;;;;;
; S6000L mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E0&MI_01
; S6000L ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E6&MI_01
; S6000L rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75EA&MI_02
; S6000L mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E4&MI_02
; S6000L bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7629&MI_01
; S6000L mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E2&MI_01

; S5000 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E5&MI_01
; S5000 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76EB&MI_01
; S5000 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76ED&MI_02
; S5000 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E9&MI_02
; S5000 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76EF&MI_01
; S5000 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E7&MI_01

; S960 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7709&MI_01
; S960 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770D&MI_01
; S960 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770F&MI_02
; S960 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770B&MI_02

; K910 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7710&MI_00
; K910 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7715&MI_01
; K910 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7717&MI_02
; K910 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7713&MI_02

; BLADE8 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F1&MI_01
; BLADE8 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F3&MI_01
; BLADE8 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F5&MI_02
; BLADE8 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F7&MI_01
; BLADE8 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F9&MI_02
; BLADE8 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FB&MI_01
; BLADE10 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FD&MI_01
; BLADE10 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FF&MI_01
; BLADE10 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7701&MI_02
; BLADE10 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7703&MI_01
; BLADE10 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7705&MI_02
; BLADE10 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7707&MI_01
; A7800 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7775&MI_00
; A7800 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_777B&MI_01
; A7800 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_777D&MI_02
; A7800 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7779&MI_02
; B8080 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7769&MI_00
; B8080 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_776F&MI_01
; B8080 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7771&MI_02
; B8080 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_776D&MI_02
; K910 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7780&MI_00
; K910 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7785&MI_01
; K910 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7787&MI_02
; K910 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7783&MI_02
; K920 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_778C&MI_00
; K920 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7791&MI_01
; K920 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7793&MI_02
; K920 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_778F&MI_02
; YOGA Tablet 2-830F mtp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7797&MI_01
; YOGA Tablet 2-830F bicr,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_779F&MI_01
; YOGA Tablet 2-1050F mtp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A3&MI_01
; YOGA Tablet 2-1050F bicr,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77AB&MI_01
; YOGA Tablet 2-830L mtp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77AF&MI_01
; YOGA Tablet 2-830L bicr,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B7&MI_01
; YOGA Tablet 2-1050L mtp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77BB&MI_01
; YOGA Tablet 2-1050L bicr,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77C3&MI_01
; YOGA Tablet 2-830L mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77AD&MI_01
; YOGA Tablet 2-830L ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B3&MI_01
; YOGA Tablet 2-830L rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B5&MI_02
; YOGA Tablet 2-830L mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B1&MI_02
; YOGA Tablet 2-830F mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7795&MI_01
; YOGA Tablet 2-830F ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_779B&MI_01
; YOGA Tablet 2-830F rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_779D&MI_02
; YOGA Tablet 2-830F mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7799&MI_02
; YOGA Tablet 2-1050L mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B9&MI_01
; YOGA Tablet 2-1050L ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77BF&MI_01
; YOGA Tablet 2-1050L rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77C1&MI_02
; YOGA Tablet 2-1050L mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77BD&MI_02
; YOGA Tablet 2-1050F mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A1&MI_01
; YOGA Tablet 2-1050F ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A7&MI_01
; YOGA Tablet 2-1050F rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A9&MI_02
; YOGA Tablet 2-1050F mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A5&MI_02
; CMCC X2 series mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_77E1&MI_01
; CMCC X2 series ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_77E5&MI_01
; CMCC X2 series rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_77E7&MI_02
; CMCC X2 series mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_77E3&MI_02
; Airplay adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F0&MI_00
; Airplay ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F5&MI_01
; Airplay rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F7&MI_02
; Airplay mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F3&MI_02
; S7 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F8&MI_00
; S7 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77FD&MI_01
; S7 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77FF&MI_02
; S7 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77FB&MI_02
; A690e adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7808&MI_00
; A690e ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_780D&MI_01
; A690e rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_780F&MI_02
; A690e mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_780B&MI_02
; A319 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7829&MI_01
; A319 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_782D&MI_01
; A319 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_782F&MI_02
; A319 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_782B&MI_02
; A320t mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7819&MI_01
; A320t ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_781D&MI_01
; A320t rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_781F&MI_02
; A320t mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_781B&MI_02
; A588t mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7821&MI_01
; A588t ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7825&MI_01
; A588t rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7827&MI_02
; A588t mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7823&MI_02
; S580 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7810&MI_00
; S580 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7815&MI_01
; S580 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7817&MI_02
; S580 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7813&MI_02
; Z2 adb,diag,modem,nmea,mass_storage,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77E8&MI_00
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77E8&MI_05
; Z2 diag,modem,nmea,mass_storage,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77E9&MI_04
; Z2 mtp,mass_storage,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EA&MI_02
; Z2 mtp,mass_storage,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77EB&MI_02
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EB&MI_03
; Z2 ptp,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EC&MI_01
; Z2 ptp,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77ED&MI_01
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77ED&MI_02
; Z2 rndis,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EE&MI_02
; Z2 rndis,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77EF&MI_02
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EF&MI_03
; Sisley adb,diag,modem,nmea,mass_storage,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7800&MI_00
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7800&MI_05
; Sisley diag,modem,nmea,mass_storage,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7801&MI_04
; Sisley mtp,mass_storage,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7802&MI_02
; Sisley mtp,mass_storage,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7803&MI_02
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7803&MI_03
; Sisley ptp,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7804&MI_01
; Sisley ptp,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7805&MI_01
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7805&MI_02
; Sisley rndis,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7806&MI_02
; Sisley rndis,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7807&MI_02
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7807&MI_03

;;;;;;;;;;;;;;;;;;;;;;CMCC USB Project end NTx86;;;;;;;;;;;;;;;;;;;;;;;;;;;

[Google.NTamd64]
;;;;;;;;;;;;;;;;;;;;;;CMCC USB history NTamd64;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
;MT65xx meta mode
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005&MI_01
;CMCC ADB Interface
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74A4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_200F
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0C03&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05c6&PID_9025&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0005
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0005&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D00D
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7495&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74EC&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7509&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05c6&PID_0001&MI_01
;;;;;;;;;;;;;;;;;;;;;;CMCC USB history end NTamd64;;;;;;;;;;;;;;;;;;;;;;;; 

;;;;;;;;;;;;;;;;;;;;;;CMCC USB Factory NTamd64;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
; Shellw rndis,diag,adb
%CompositeAdbInterface% = USB_Install, USB\VID_05C6&PID_902D&MI_03
;;;;;;;;;;;;;;;;;;;;;;CMCC USB Factory end NTamd64;;;;;;;;;;;;;;;;;;;;;;;;;;;; 

;;;;;;;;;;;;;;;;;;;;;;CMCC USB generic NTamd64;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
;generic mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7435&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2009&MI_01
;generic mass_storage,adb,acm
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74ED&MI_01
;generic adb,diag,modem,nmea
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7501&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_200D&MI_00
;generic adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7513&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2000&MI_00
;generic mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F8&MI_01
;generic ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2005&MI_01
;generic rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7500&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2003&MI_02
;generic bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750E&MI_01
;generic mtp,adb,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74EE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_200C&MI_01
;generic mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7718&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2008&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_2B76&PID_2006&MI_02
;;;;;;;;;;;;;;;;;;;;;;CMCC USB generic end NTamd64;;;;;;;;;;;;;;;;;;;;;;;;; 
      
;;;;;;;;;;;;;;;;;;;;;;CMCC USB Project NTamd64;;;;;;;;;;;;;;;;;;;;;;;;;;;
; S6000L mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E0&MI_01
; S6000L ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E6&MI_01
; S6000L rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75EA&MI_02
; S6000L mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E4&MI_02
; S6000L bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7629&MI_01
; S6000L mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E2&MI_01
; S5000 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E5&MI_01
; S5000 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76EB&MI_01
; S5000 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76ED&MI_02
; S5000 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E9&MI_02
; S5000 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76EF&MI_01
; S5000 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E7&MI_01
; S960 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7709&MI_01
; S960 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770D&MI_01
; S960 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770F&MI_02
; S960 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770B&MI_02
; K910 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7710&MI_00
; K910 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7715&MI_01
; K910 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7717&MI_02
; K910 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7713&MI_02
; BLADE8 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F1&MI_01
; BLADE8 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F3&MI_01
; BLADE8 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F5&MI_02
; BLADE8 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F7&MI_01
; BLADE8 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F9&MI_02
; BLADE8 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FB&MI_01
; BLADE10 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FD&MI_01
; BLADE10 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FF&MI_01
; BLADE10 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7701&MI_02
; BLADE10 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7703&MI_01
; BLADE10 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7705&MI_02
; BLADE10 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7707&MI_01
; A7800 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7775&MI_00
; A7800 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_777B&MI_01
; A7800 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_777D&MI_02
; A7800 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7779&MI_02
; B8080 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7769&MI_00
; B8080 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_776F&MI_01
; B8080 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7771&MI_02
; B8080 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_776D&MI_02
; K910 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7780&MI_00
; K910 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7785&MI_01
; K910 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7787&MI_02
; K910 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7783&MI_02
; K920 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_778C&MI_00
; K920 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7791&MI_01
; K920 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7793&MI_02
; K920 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_778F&MI_02
; YOGA Tablet 2-830F mtp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7797&MI_01
; YOGA Tablet 2-830F bicr,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_779F&MI_01
; YOGA Tablet 2-1050F mtp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A3&MI_01
; YOGA Tablet 2-1050F bicr,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77AB&MI_01
; YOGA Tablet 2-830L mtp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77AF&MI_01
; YOGA Tablet 2-830L bicr,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B7&MI_01
; YOGA Tablet 2-1050L mtp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77BB&MI_01
; YOGA Tablet 2-1050L bicr,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77C3&MI_01
; YOGA Tablet 2-830L mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77AD&MI_01
; YOGA Tablet 2-830L ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B3&MI_01
; YOGA Tablet 2-830L rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B5&MI_02
; YOGA Tablet 2-830L mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B1&MI_02
; YOGA Tablet 2-830F mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7795&MI_01
; YOGA Tablet 2-830F ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_779B&MI_01
; YOGA Tablet 2-830F rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_779D&MI_02
; YOGA Tablet 2-830F mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7799&MI_02
; YOGA Tablet 2-1050L mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77B9&MI_01
; YOGA Tablet 2-1050L ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77BF&MI_01
; YOGA Tablet 2-1050L rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77C1&MI_02
; YOGA Tablet 2-1050L mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77BD&MI_02
; YOGA Tablet 2-1050F mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A1&MI_01
; YOGA Tablet 2-1050F ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A7&MI_01
; YOGA Tablet 2-1050F rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A9&MI_02
; YOGA Tablet 2-1050F mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77A5&MI_02
; CMCC X2 series mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_77E1&MI_01
; CMCC X2 series ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_77E5&MI_01
; CMCC X2 series rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_77E7&MI_02
; CMCC X2 series mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_77E3&MI_02
; Airplay adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F0&MI_00
; Airplay ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F5&MI_01
; Airplay rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F7&MI_02
; Airplay mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F3&MI_02
; S7 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77F8&MI_00
; S7 ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77FD&MI_01
; S7 rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77FF&MI_02
; S7 mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77FB&MI_02
; A690e adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7808&MI_00
; A690e ptp,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_780D&MI_01
; A690e rndis,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_780F&MI_02
; A690e mtp,mass_storage,adb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_780B&MI_02
; A319 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7829&MI_01
; A319 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_782D&MI_01
; A319 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_782F&MI_02
; A319 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_782B&MI_02
; A320t mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7819&MI_01
; A320t ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_781D&MI_01
; A320t rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_781F&MI_02
; A320t mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_781B&MI_02
; A588t mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7821&MI_01
; A588t ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7825&MI_01
; A588t rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7827&MI_02
; A588t mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7823&MI_02
; S580 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7810&MI_00
; S580 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7815&MI_01
; S580 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7817&MI_02
; S580 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7813&MI_02
; Z2 adb,diag,modem,nmea,mass_storage,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77E8&MI_00
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77E8&MI_05
; Z2 diag,modem,nmea,mass_storage,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77E9&MI_04
; Z2 mtp,mass_storage,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EA&MI_02
; Z2 mtp,mass_storage,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77EB&MI_02
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EB&MI_03
; Z2 ptp,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EC&MI_01
; Z2 ptp,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77ED&MI_01
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77ED&MI_02
; Z2 rndis,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EE&MI_02
; Z2 rndis,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_77EF&MI_02
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_77EF&MI_03
; Sisley adb,diag,modem,nmea,mass_storage,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7800&MI_00
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7800&MI_05
; Sisley diag,modem,nmea,mass_storage,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7801&MI_04
; Sisley mtp,mass_storage,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7802&MI_02
; Sisley mtp,mass_storage,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7803&MI_02
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7803&MI_03
; Sisley ptp,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7804&MI_01
; Sisley ptp,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7805&MI_01
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7805&MI_02
; Sisley rndis,ldb
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7806&MI_02
; Sisley rndis,adb,ldb
%CompositeAdbInterface% = USB_Install, USB\VID_17EF&PID_7807&MI_02
%CompositeLdbInterface% = USB_Install, USB\VID_17EF&PID_7807&MI_03
;;;;;;;;;;;;;;;;;;;;;;CMCC USB Project end NTamd64;;;;;;;;;;;;;;;;;;;;;;;;;;;

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion  = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 2
WdfCoInstaller01009.dll = 2

[Strings]
ProviderName                = "CMCC Inc."
SingleAdbInterface          = "CMCC ADB Interface"
CompositeAdbInterface       = "CMCC Composite ADB Interface"
CompositeLdbInterface       = "CMCC Composite LDB Interface"
SingleBootLoaderInterface   = "CMCC Bootloader Interface"
WinUSB_SvcDesc              = "CMCC USB Driver"
DISK_NAME                   = "CMCC WinUsb installation disk"
ClassName                   = "CMCC ADB Device"