;*****************************************************************************
;
; Copyright 2010 Ericsson AB
;
;*****************************************************************************

[Version]
signature="$WINDOWS NT$"
Class=Modem
ClassGuid={4d36e96d-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
DriverVer=08/09/2010,5.24.1.0
CatalogFile=e36wmdmts.cat

[ControlFlags]
ExcludeFromSelect = *

[SourceDisksNames.x86]
; diskid = description[, [tagfile] [, <unused>, subdir]]
1=%DiskString%,"Mbm4mdm.sys",,\i386

[SourceDisksNames.amd64]
; diskid = description[, [tagfile] [, <unused>, subdir]]
1=%DiskString%,"Mbm4mdm.sys",,\amd64


[SourceDisksFiles]
; filename = diskid[,[ subdir][, size]]
Mbm4mdm.sys = 1
Mbm4cmnt.sys = 1
Mbm4mdfl.sys = 1
MbmFilter.sys = 1
WdfCoInstaller01009.dll = 1

;-----------------------------------------------------------------------------
; Specify target paths...
;-----------------------------------------------------------------------------

[DestinationDirs]
DefaultDestDir = 12                    ; system32\drivers

;-----------------------------------------------------------------------------
; Table of Contents
;-----------------------------------------------------------------------------
[Manufacturer]
%Ericsson%=e36w, NTamd64

;-----------------------------------------------------------------------------
; Device-by-device entries
;-----------------------------------------------------------------------------
[e36w]
%e36w.Modem.Desc% = VID_0bdb&PID_1904.Install, USB\VID_0bdb&PID_1904&MI_01&OS_NT
%e36w.Modem.Desc2% = VID_0bdb&PID_1904.Install, USB\VID_0bdb&PID_1904&MI_03&OS_NT
%e36w.Modem.Desc% = VID_0bdb&PID_1906.Install, USB\VID_0bdb&PID_1906&MI_01&OS_NT
%e36w.Modem.Desc2% = VID_0bdb&PID_1906.Install, USB\VID_0bdb&PID_1906&MI_03&OS_NT
%e36w.Modem.Desc.2% = VID_0bdb&PID_1909.Install, USB\VID_0bdb&PID_1909&MI_01&OS_NT
%e36w.Modem.Desc2.2% = VID_0bdb&PID_1909.Install, USB\VID_0bdb&PID_1909&MI_03&OS_NT
%e36w.Modem.Desc.2% = VID_0bdb&PID_190A.Install, USB\VID_0bdb&PID_190A&MI_01&OS_NT
%e36w.Modem.Desc2.2% = VID_0bdb&PID_190A.Install, USB\VID_0bdb&PID_190A&MI_03&OS_NT
%e36w.Modem.Desc.2% = VID_0bdb&PID_1914.Install, USB\VID_0bdb&PID_1914&MI_01&OS_NT
%e36w.Modem.Desc2.2% = VID_0bdb&PID_1914.Install, USB\VID_0bdb&PID_1914&MI_03&OS_NT
%e36w.Modem.Desc.3% = VID_0bdb&PID_190D.Install, USB\VID_0bdb&PID_190D&MI_01&OS_NT
%e36w.Modem.Desc2.3% = VID_0bdb&PID_190D.Install, USB\VID_0bdb&PID_190D&MI_03&OS_NT
%e36w.Modem.Desc.4% = VID_0bdb&PID_1045.Install, USB\VID_0bdb&PID_1045&MI_01&OS_NT
%e36w.Modem.Desc2.4% = VID_0bdb&PID_1045.Install, USB\VID_0bdb&PID_1045&MI_03&OS_NT

[e36w.NTamd64]
%e36w.Modem.Desc% = VID_0bdb&PID_1904.Install, USB\VID_0bdb&PID_1904&MI_01&OS_NT
%e36w.Modem.Desc2% = VID_0bdb&PID_1904.Install, USB\VID_0bdb&PID_1904&MI_03&OS_NT
%e36w.Modem.Desc% = VID_0bdb&PID_1906.Install, USB\VID_0bdb&PID_1906&MI_01&OS_NT
%e36w.Modem.Desc2% = VID_0bdb&PID_1906.Install, USB\VID_0bdb&PID_1906&MI_03&OS_NT
%e36w.Modem.Desc.2% = VID_0bdb&PID_1909.Install, USB\VID_0bdb&PID_1909&MI_01&OS_NT
%e36w.Modem.Desc2.2% = VID_0bdb&PID_1909.Install, USB\VID_0bdb&PID_1909&MI_03&OS_NT
%e36w.Modem.Desc.2% = VID_0bdb&PID_190A.Install, USB\VID_0bdb&PID_190A&MI_01&OS_NT
%e36w.Modem.Desc2.2% = VID_0bdb&PID_190A.Install, USB\VID_0bdb&PID_190A&MI_03&OS_NT
%e36w.Modem.Desc.2% = VID_0bdb&PID_1914.Install, USB\VID_0bdb&PID_1914&MI_01&OS_NT
%e36w.Modem.Desc2.2% = VID_0bdb&PID_1914.Install, USB\VID_0bdb&PID_1914&MI_03&OS_NT
%e36w.Modem.Desc.3% = VID_0bdb&PID_190D.Install, USB\VID_0bdb&PID_190D&MI_01&OS_NT
%e36w.Modem.Desc2.3% = VID_0bdb&PID_190D.Install, USB\VID_0bdb&PID_190D&MI_03&OS_NT
%e36w.Modem.Desc.4% = VID_0bdb&PID_1045.Install, USB\VID_0bdb&PID_1045&MI_01&OS_NT
%e36w.Modem.Desc2.4% = VID_0bdb&PID_1045.Install, USB\VID_0bdb&PID_1045&MI_03&OS_NT

;-----------------------------------------------------------------------------
; Installation instructions
;-----------------------------------------------------------------------------

[VID_0bdb&PID_1904.Install.nt]
AddReg = VID_0bdb&PID_1904.AddReg, VID_0bdb&PID_1904.NT.AddReg, GenericAddReg, USB
CopyFiles	= CopyFiles, CopyFiles.Win2K
[VID_0bdb&PID_1906.Install.nt]
AddReg = VID_0bdb&PID_1906.AddReg, VID_0bdb&PID_1906.NT.AddReg, GenericAddReg, USB
CopyFiles	= CopyFiles, CopyFiles.Win2K
[VID_0bdb&PID_1909.Install.nt]
AddReg = VID_0bdb&PID_1909.AddReg, VID_0bdb&PID_1909.NT.AddReg, GenericAddReg, USB
CopyFiles	= CopyFiles, CopyFiles.Win2K
[VID_0bdb&PID_190A.Install.nt]
AddReg = VID_0bdb&PID_190A.AddReg, VID_0bdb&PID_190A.NT.AddReg, GenericAddReg, USB
CopyFiles	= CopyFiles, CopyFiles.Win2K
[VID_0bdb&PID_1914.Install.nt]
AddReg = VID_0bdb&PID_1914.AddReg, VID_0bdb&PID_1914.NT.AddReg, GenericAddReg, USB
CopyFiles	= CopyFiles, CopyFiles.Win2K
[VID_0bdb&PID_190D.Install.nt]
AddReg = VID_0bdb&PID_190D.AddReg, VID_0bdb&PID_190D.NT.AddReg, GenericAddReg, USB
CopyFiles	= CopyFiles, CopyFiles.Win2K
[VID_0bdb&PID_1045.Install.nt]
AddReg = VID_0bdb&PID_1045.AddReg, VID_0bdb&PID_1045.NT.AddReg, GenericAddReg, USB
CopyFiles	= CopyFiles, CopyFiles.Win2K

;-----------------------------------------------------------------------------
;  Registry
;-----------------------------------------------------------------------------

[VID_0bdb&PID_1904.AddReg]
HKR,,NTMPDriver,,Mbm4mdm.sys
HKR,,Properties,  1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 01,00,00,00, 00,dd,6d,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,dd,6d,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,OverrideDefaultPortSettings, 0x10001, 01,00,00,00
HKR,,InitialBaudRate, 0x10001, 00,dd,6d,00
HKR,,InitialLineControl,, "8N1"					;8-bits, No parity, 1 stop bit
HKR,,EnableSetClearFeatureIdle, 0x10001, 01,00,00,00
[VID_0bdb&PID_1906.AddReg]
HKR,,NTMPDriver,,Mbm4mdm.sys
HKR,,Properties,  1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 01,00,00,00, 00,dd,6d,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,dd,6d,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,OverrideDefaultPortSettings, 0x10001, 01,00,00,00
HKR,,InitialBaudRate, 0x10001, 00,dd,6d,00
HKR,,InitialLineControl,, "8N1"					;8-bits, No parity, 1 stop bit
HKR,,EnableSetClearFeatureIdle, 0x10001, 01,00,00,00
[VID_0bdb&PID_1909.AddReg]
HKR,,NTMPDriver,,Mbm4mdm.sys
HKR,,Properties,  1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 01,00,00,00, 00,dd,6d,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,dd,6d,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,OverrideDefaultPortSettings, 0x10001, 01,00,00,00
HKR,,InitialBaudRate, 0x10001, 00,dd,6d,00
HKR,,InitialLineControl,, "8N1"					;8-bits, No parity, 1 stop bit
HKR,,EnableSetClearFeatureIdle, 0x10001, 01,00,00,00
[VID_0bdb&PID_190A.AddReg]
HKR,,NTMPDriver,,Mbm4mdm.sys
HKR,,Properties,  1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 01,00,00,00, 00,dd,6d,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,dd,6d,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,OverrideDefaultPortSettings, 0x10001, 01,00,00,00
HKR,,InitialBaudRate, 0x10001, 00,dd,6d,00
HKR,,InitialLineControl,, "8N1"					;8-bits, No parity, 1 stop bit
HKR,,EnableSetClearFeatureIdle, 0x10001, 01,00,00,00
[VID_0bdb&PID_1914.AddReg]
HKR,,NTMPDriver,,Mbm4mdm.sys
HKR,,Properties,  1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 01,00,00,00, 00,dd,6d,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,dd,6d,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,OverrideDefaultPortSettings, 0x10001, 01,00,00,00
HKR,,InitialBaudRate, 0x10001, 00,dd,6d,00
HKR,,InitialLineControl,, "8N1"					;8-bits, No parity, 1 stop bit
HKR,,EnableSetClearFeatureIdle, 0x10001, 01,00,00,00
[VID_0bdb&PID_190D.AddReg]
HKR,,NTMPDriver,,Mbm4mdm.sys
HKR,,Properties,  1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 01,00,00,00, 40,6F,40,01, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 40,6F,40,01, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,OverrideDefaultPortSettings, 0x10001, 01,00,00,00
HKR,,InitialBaudRate, 0x10001, 40,6F,40,01
HKR,,InitialLineControl,, "8N1"					;8-bits, No parity, 1 stop bit
HKR,,EnableSetClearFeatureIdle, 0x10001, 01,00,00,00
[VID_0bdb&PID_1045.AddReg]
HKR,,NTMPDriver,,Mbm4mdm.sys
HKR,,Properties,  1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 01,00,00,00, 00,dd,6d,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,dd,6d,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,OverrideDefaultPortSettings, 0x10001, 01,00,00,00
HKR,,InitialBaudRate, 0x10001, 00,dd,6d,00
HKR,,InitialLineControl,, "8N1"					;8-bits, No parity, 1 stop bit
HKR,,EnableSetClearFeatureIdle, 0x10001, 01,00,00,00

; only for NT...
[VID_0bdb&PID_1904.NT.AddReg]
HKR,,EnableCR3840, 0x10001, 01,00,00,00
HKR,,AllowSuspendWhileOpen, 0x10001, 01,00,00,00
HKR,,AllowRemoteWakeup, 0x10001, 01,00,00,00
HKR,,EnableSelectiveSuspendHeuristics, 0x10001, 05,00,00,00
HKR,,EnableSelectiveSuspend, 0x10001, 01, 00, 00, 00
; only for NT...
[VID_0bdb&PID_1906.NT.AddReg]
HKR,,EnableCR3840, 0x10001, 01,00,00,00
HKR,,AllowSuspendWhileOpen, 0x10001, 01,00,00,00
HKR,,AllowRemoteWakeup, 0x10001, 01,00,00,00
HKR,,EnableSelectiveSuspendHeuristics, 0x10001, 05,00,00,00
HKR,,EnableSelectiveSuspend, 0x10001, 01, 00, 00, 00
; only for NT...
[VID_0bdb&PID_1909.NT.AddReg]
HKR,,EnableCR3840, 0x10001, 01,00,00,00
HKR,,AllowSuspendWhileOpen, 0x10001, 01,00,00,00
HKR,,AllowRemoteWakeup, 0x10001, 01,00,00,00
HKR,,EnableSelectiveSuspendHeuristics, 0x10001, 05,00,00,00
HKR,,EnableSelectiveSuspend, 0x10001, 01, 00, 00, 00
; only for NT...
[VID_0bdb&PID_190A.NT.AddReg]
HKR,,EnableCR3840, 0x10001, 01,00,00,00
HKR,,AllowSuspendWhileOpen, 0x10001, 01,00,00,00
HKR,,AllowRemoteWakeup, 0x10001, 01,00,00,00
HKR,,EnableSelectiveSuspendHeuristics, 0x10001, 05,00,00,00
HKR,,EnableSelectiveSuspend, 0x10001, 01, 00, 00, 00
; only for NT...
[VID_0bdb&PID_1914.NT.AddReg]
HKR,,EnableCR3840, 0x10001, 01,00,00,00
HKR,,AllowSuspendWhileOpen, 0x10001, 01,00,00,00
HKR,,AllowRemoteWakeup, 0x10001, 01,00,00,00
HKR,,EnableSelectiveSuspendHeuristics, 0x10001, 05,00,00,00
HKR,,EnableSelectiveSuspend, 0x10001, 01, 00, 00, 00
; only for NT...
[VID_0bdb&PID_190D.NT.AddReg]
HKR,,EnableCR3840, 0x10001, 01,00,00,00
HKR,,AllowSuspendWhileOpen, 0x10001, 01,00,00,00
HKR,,AllowRemoteWakeup, 0x10001, 01,00,00,00
HKR,,EnableSelectiveSuspendHeuristics, 0x10001, 05,00,00,00
HKR,,EnableSelectiveSuspend, 0x10001, 01, 00, 00, 00
; only for NT...
[VID_0bdb&PID_1045.NT.AddReg]
HKR,,EnableCR3840, 0x10001, 01,00,00,00
HKR,,AllowSuspendWhileOpen, 0x10001, 01,00,00,00
HKR,,AllowRemoteWakeup, 0x10001, 01,00,00,00
HKR,,EnableSelectiveSuspendHeuristics, 0x10001, 05,00,00,00
HKR,,EnableSelectiveSuspend, 0x10001, 01, 00, 00, 00


;-----------------------------------------------------------------------------
;  Copy lists
;-----------------------------------------------------------------------------
[CopyFiles]

[CopyFiles.Win2K]
Mbm4mdm.sys
Mbm4cm.sys,Mbm4cmnt.sys
Mbm4cmnt.sys
Mbm4mdfl.sys
MbmFilter.sys
WdfCoInstaller01009.dll



;-----------------------------------------------------------------------------
;  NT Services installation
;-----------------------------------------------------------------------------

; only for NT...
[VID_0bdb&PID_1904.Install.NT.HW]
AddReg = LowerFilterAddReg
AddReg = UpperFilterAddReg
; only for NT...
[VID_0bdb&PID_1906.Install.NT.HW]
AddReg = LowerFilterAddReg
AddReg = UpperFilterAddReg
; only for NT...
[VID_0bdb&PID_1909.Install.NT.HW]
AddReg = LowerFilterAddReg
AddReg = UpperFilterAddReg
; only for NT...
[VID_0bdb&PID_190A.Install.NT.HW]
AddReg = LowerFilterAddReg
AddReg = UpperFilterAddReg
; only for NT...
[VID_0bdb&PID_1914.Install.NT.HW]
AddReg = LowerFilterAddReg
AddReg = UpperFilterAddReg
; only for NT...
[VID_0bdb&PID_190D.Install.NT.HW]
AddReg = LowerFilterAddReg
AddReg = UpperFilterAddReg
; only for NT...
[VID_0bdb&PID_1045.Install.NT.HW]
AddReg = LowerFilterAddReg
AddReg = UpperFilterAddReg

[VID_0bdb&PID_1904.Install.NT.Services]
AddService = Mbm4mdm, 0x00000000, e36w.Install.AddService, e36w.Install.EventLog
AddService = Mbm4mdfl,, e36w.Install.AddFilter
AddService = MbmFilter,, e36w.Install.AddFilter_MBM
[VID_0bdb&PID_1906.Install.NT.Services]
AddService = Mbm4mdm, 0x00000000, e36w.Install.AddService, e36w.Install.EventLog
AddService = Mbm4mdfl,, e36w.Install.AddFilter
AddService = MbmFilter,, e36w.Install.AddFilter_MBM
[VID_0bdb&PID_1909.Install.NT.Services]
AddService = Mbm4mdm, 0x00000000, e36w.Install.AddService, e36w.Install.EventLog
AddService = Mbm4mdfl,, e36w.Install.AddFilter
AddService = MbmFilter,, e36w.Install.AddFilter_MBM
[VID_0bdb&PID_190A.Install.NT.Services]
AddService = Mbm4mdm, 0x00000000, e36w.Install.AddService, e36w.Install.EventLog
AddService = Mbm4mdfl,, e36w.Install.AddFilter
AddService = MbmFilter,, e36w.Install.AddFilter_MBM
[VID_0bdb&PID_1914.Install.NT.Services]
AddService = Mbm4mdm, 0x00000000, e36w.Install.AddService, e36w.Install.EventLog
AddService = Mbm4mdfl,, e36w.Install.AddFilter
AddService = MbmFilter,, e36w.Install.AddFilter_MBM
[VID_0bdb&PID_190D.Install.NT.Services]
AddService = Mbm4mdm, 0x00000000, e36w.Install.AddService, e36w.Install.EventLog
AddService = Mbm4mdfl,, e36w.Install.AddFilter
AddService = MbmFilter,, e36w.Install.AddFilter_MBM
[VID_0bdb&PID_1045.Install.NT.Services]
AddService = Mbm4mdm, 0x00000000, e36w.Install.AddService, e36w.Install.EventLog
AddService = Mbm4mdfl,, e36w.Install.AddFilter
AddService = MbmFilter,, e36w.Install.AddFilter_MBM

[UpperFilterAddReg]
HKR,,"UpperFilters",0x00010000,"Mbm4mdfl"
HKR,,"UpperFilters",0x00010008,"MbmFilter"

[e36w.Install.AddService]
DisplayName	= %e36w.Service.Name%
Description	= %e36w.Service.Desc%
ServiceType	= 1			;%SERVICE_KERNEL_DRIVER%
StartType	= 3			;%SERVICE_DEMAND_START%
ErrorControl	= 1			;%SERVICE_ERROR_NORMAL%	
ServiceBinary	= %12%\Mbm4mdm.sys

[e36w.Install.AddFilter]
DisplayName	= %e36w.Filter.Name%
Description	= %e36w.Filter.Desc%
ServiceType	= 1			;%SERVICE_KERNEL_DRIVER%
StartType	= 3			;%SERVICE_DEMAND_START%
ErrorControl	= 1			;%SERVICE_ERROR_NORMAL%	
ServiceBinary	= %12%\Mbm4mdfl.sys

[e36w.Install.AddFilter_MBM]
DisplayName	= %e36w.Filter.Name_MBM%
Description	= %e36w.Filter.Desc_MBM%
ServiceType	= 1			;%SERVICE_KERNEL_DRIVER%
StartType	= 3			;%SERVICE_DEMAND_START%
ErrorControl	= 1			;%SERVICE_ERROR_NORMAL%	
ServiceBinary	= %12%\MbmFilter.sys

; ================= WDF co-Installer section =====================

[VID_0bdb&PID_1904.Install.NT.CoInstallers]
AddReg    = MbmFilter_AddReg
CopyFiles = MbmFilter_CopyFiles
[VID_0bdb&PID_1906.Install.NT.CoInstallers]
AddReg    = MbmFilter_AddReg
CopyFiles = MbmFilter_CopyFiles
[VID_0bdb&PID_1909.Install.NT.CoInstallers]
AddReg    = MbmFilter_AddReg
CopyFiles = MbmFilter_CopyFiles
[VID_0bdb&PID_190A.Install.NT.CoInstallers]
AddReg    = MbmFilter_AddReg
CopyFiles = MbmFilter_CopyFiles
[VID_0bdb&PID_1914.Install.NT.CoInstallers]
AddReg    = MbmFilter_AddReg
CopyFiles = MbmFilter_CopyFiles
[VID_0bdb&PID_190D.Install.NT.CoInstallers]
AddReg    = MbmFilter_AddReg
CopyFiles = MbmFilter_CopyFiles
[VID_0bdb&PID_1045.Install.NT.CoInstallers]
AddReg    = MbmFilter_AddReg
CopyFiles = MbmFilter_CopyFiles

[DestinationDirs]
MbmFilter_CopyFiles = 11

[MbmFilter_CopyFiles]
WdfCoInstaller01009.dll

[MbmFilter_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"

[VID_0bdb&PID_1904.Install.NT.Wdf]
KmdfService  = MbmFilter, VID_0bdb&PID_1904.Install.NT.Wdf.Install
[VID_0bdb&PID_1906.Install.NT.Wdf]
KmdfService  = MbmFilter, VID_0bdb&PID_1906.Install.NT.Wdf.Install
[VID_0bdb&PID_1909.Install.NT.Wdf]
KmdfService  = MbmFilter, VID_0bdb&PID_1909.Install.NT.Wdf.Install
[VID_0bdb&PID_190A.Install.NT.Wdf]
KmdfService  = MbmFilter, VID_0bdb&PID_190A.Install.NT.Wdf.Install
[VID_0bdb&PID_1914.Install.NT.Wdf]
KmdfService  = MbmFilter, VID_0bdb&PID_1914.Install.NT.Wdf.Install
[VID_0bdb&PID_190D.Install.NT.Wdf]
KmdfService  = MbmFilter, VID_0bdb&PID_190D.Install.NT.Wdf.Install
[VID_0bdb&PID_1045.Install.NT.Wdf]
KmdfService  = MbmFilter, VID_0bdb&PID_1045.Install.NT.Wdf.Install

[VID_0bdb&PID_1904.Install.NT.Wdf.Install]
KmdfLibraryVersion = 1.9
[VID_0bdb&PID_1906.Install.NT.Wdf.Install]
KmdfLibraryVersion = 1.9
[VID_0bdb&PID_1909.Install.NT.Wdf.Install]
KmdfLibraryVersion = 1.9
[VID_0bdb&PID_190A.Install.NT.Wdf.Install]
KmdfLibraryVersion = 1.9
[VID_0bdb&PID_1914.Install.NT.Wdf.Install]
KmdfLibraryVersion = 1.9
[VID_0bdb&PID_190D.Install.NT.Wdf.Install]
KmdfLibraryVersion = 1.9
[VID_0bdb&PID_1045.Install.NT.Wdf.Install]
KmdfLibraryVersion = 1.9

;-----------------------------------------------------------------------------
;       Event logging support
;-----------------------------------------------------------------------------

[e36w.Install.EventLog]
Addreg = e36w.EventLog.AddReg

[e36w.EventLog.AddReg]
HKR,,EventMessageFile, 0x20000, "%%SystemRoot%%\System32\drivers\Mbm4mdm.sys"
HKR,,TypesSupported, 0x10001, 7

;-----------------------------------------------------------------------------
[LowerFilterAddReg]
HKR,,"LowerFilters",0x00010000,"Mbm4mdm"

[GenericAddReg]
HKR,, FriendlyDriver,,unimodem.vxd
HKR,, PortSubClass,1, 02
HKR,, ConfigDialog,, modemui.dll
HKR,, EnumPropPages,, "modemui.dll,EnumPropPages"
HKR,, FClass, 1, c3,00,00,00
;HKR,, VoiceProfile,    1,23,22,09,00
HKR, Fax, CL1FCS,, "2"

HKR, Init, 1,, "AT<cr>"
HKR, Init, 2,, "AT &F<cr>"
HKR, Init, 3,, "AT V1E0S0=0&D2&C1<cr>"
HKR, Init, 4,, "AT +CMEE=1<cr>"
HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 2,, "None"
HKR, Answer, 1,, "ATA<cr>"
HKR, Hangup, 1,, "ATH<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Settings, Compression_Off,, "+DS=0;+DR=0;"
HKR, Settings, Compression_On,, "+DS=3,0,2048,32;+DR=1;"
HKR, Settings, CompatibilityFlags, 1, 01 ,00 ,00, 00
HKR, Settings, CallSetupFailTimer,, "S7=<#>;"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ";"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"


; DTE/DCE speeds will not be exact for generic modems because we will
; treat CONNECT as a DCE speed when some modems will report it as DTE.
HKR, Responses, "0<cr>",    1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK - Command executed
HKR, Responses, "1<cr>",    1, 02, 00, 00,00,00,00, 00,00,00,00 ; CONNECT - Connection
HKR, Responses, "2<cr>",    1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING - Ring signal indicated
HKR, Responses, "3<cr>",    1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER 
HKR, Responses, "4<cr>",    1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR - Invalid command
HKR, Responses, "5<cr>",    1, 02, 00, B0,04,00,00, 00,00,00,00 ; CONNECT 1200
HKR, Responses, "6<cr>",    1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE - No dial tone detected
HKR, Responses, "7<cr>",    1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY - Engaged (busy) signal
HKR, Responses, "8<cr>",    1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER

HKR, Responses, "<cr><lf>OK<cr><lf>",                     1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",                   1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",             1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",                  1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>",            1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIAL TONE<cr><lf>",           1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",                   1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",              1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",                1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",           1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",           1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",           1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>",          1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",          1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800<cr><lf>",          1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600<cr><lf>",          1, 02, 00, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",          1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",          1, 02, 00, 00,e1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",         1, 02, 00, 00,c2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 230400<cr><lf>",         1, 02, 00, 00,84,03,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 460800<cr><lf>",         1, 02, 00, 00,08,07,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 3686400<cr><lf>",        1, 02, 00, 00,40,38,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200000<cr><lf>",        1, 02, 00, 00,dd,6d,00, 00,00,00,00
HKR, Responses, "<cr><lf>FAX<cr><lf>",                    1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATA<cr><lf>",                   1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>VOICE<cr><lf>",                  1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RINGING<cr><lf>",                1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DELAYED<cr><lf>",                1, 1D, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DELAYED NUMBER<cr><lf>",         1, 1D, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BLACKLISTED<cr><lf>",            1, 1C, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BLACKLISTED NUMBER<cr><lf>",     1, 1C, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+FCERROR<cr><lf>",               1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+DR: NONE<cr><lf>",              1, 02, 00, 00,00,00,00, 00,00,00,00   ; No compression
HKR, Responses, "<cr><lf>+DR: V42B<cr><lf>",              1, 02, 03, 00,00,00,00, 00,00,00,00   ; Compression enabled

HKR, Responses, "<cr><lf>+CME ERROR: 0<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Phone failure.
HKR, Responses, "<cr><lf>+CME ERROR: 1<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; No connection to phone.
HKR, Responses, "<cr><lf>+CME ERROR: 2<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Phone modem link reserved.
HKR, Responses, "<cr><lf>+CME ERROR: 3<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Operation not permitted.
HKR, Responses, "<cr><lf>+CME ERROR: 4<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Operation not supported.
HKR, Responses, "<cr><lf>+CME ERROR: 5<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; PH-SIM card PIN required.
HKR, Responses, "<cr><lf>+CME ERROR: 6<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; PH-FSIM PIN required
HKR, Responses, "<cr><lf>+CME ERROR: 7<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; PH-FSIM PUK required
HKR, Responses, "<cr><lf>+CME ERROR: 10<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card not inserted.
HKR, Responses, "<cr><lf>+CME ERROR: 11<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card PIN required.
HKR, Responses, "<cr><lf>+CME ERROR: 12<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card PUK required.
HKR, Responses, "<cr><lf>+CME ERROR: 13<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card failure.
HKR, Responses, "<cr><lf>+CME ERROR: 14<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card busy.
HKR, Responses, "<cr><lf>+CME ERROR: 15<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card wrong.
HKR, Responses, "<cr><lf>+CME ERROR: 16<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Incorrect password.
HKR, Responses, "<cr><lf>+CME ERROR: 20<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Memory full.
HKR, Responses, "<cr><lf>+CME ERROR: 21<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Invalid index.
HKR, Responses, "<cr><lf>+CME ERROR: 22<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Not found.
HKR, Responses, "<cr><lf>+CME ERROR: 23<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Memory failure.
HKR, Responses, "<cr><lf>+CME ERROR: 24<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Text string too long.
HKR, Responses, "<cr><lf>+CME ERROR: 25<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Invalid character in text string.
HKR, Responses, "<cr><lf>+CME ERROR: 26<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Dial string too long.
HKR, Responses, "<cr><lf>+CME ERROR: 27<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Invalid character in dial string.
HKR, Responses, "<cr><lf>+CME ERROR: 30<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; No network service
HKR, Responses, "<cr><lf>+CME ERROR: 31<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Network timeout
HKR, Responses, "<cr><lf>+CME ERROR: 100<cr><lf>",  1, 03, 00, 00,00,00,00, 00,00,00,00   ; Unknown.
HKR, Responses, "<cr><lf>+CMS ERROR: ",             1, 03, 00, 00,00,00,00, 00,00,00,00   ; CMS errors


[USB]
HKR,, PortDriver, 0, wdmmdmld.vxd
HKR,, DeviceType, 1, 01


;-----------------------------------------------------------------------------
; STRINGS
;-----------------------------------------------------------------------------
[Strings]

;<<localize the following>>

;BEGIN ENG - US English Strings

Provider = "Ericsson AB"
Ericsson = "Ericsson AB"
e36w.Modem.Desc = "F3607gw Mobile Broadband Modem"
e36w.Modem.Desc2 = "F3607gw Mobile Broadband Data Modem"
e36w.Modem.Desc.2 = "F3307 Mobile Broadband Modem"
e36w.Modem.Desc2.2 = "F3307 Mobile Broadband Data Modem"
e36w.Modem.Desc.3 = "F5521gw Mobile Broadband Modem"
e36w.Modem.Desc2.3 = "F5521gw Mobile Broadband Data Modem"
e36w.Modem.Desc.4 = "Ericsson Mobile Broadband Modem"
e36w.Modem.Desc2.4 = "Ericsson Mobile Broadband Data Modem"

e36w.Service.Name = " Mobile Broadband Data Modem Driver"
e36w.Service.Desc = " Mobile Broadband Data Modem Driver"
e36w.Filter.Name = " Mobile Broadband Data Modem Filter"
e36w.Filter.Desc = " Mobile Broadband Data Modem Filter"

e36w.Filter.Name_MBM = "Ericsson MBM Modem Filter Driver"
e36w.Filter.Desc_MBM = "Ericsson MBM Modem Filter Driver"

DiskString = " Mobile Broadband Data Modem Installation Disk"
CustomerDataPath = " Mobile Broadband Device"
DriverSet = " Mobile Broadband Device Software"
UninstallFile = "MBM4Uninstall.exe"
McciOptions = "Uninstallable"


;END ENG - US English Strings

;-----------------------------------------------------------------------------
; The following are symbolic constants which don't change per locale.
;-----------------------------------------------------------------------------


;*** end of file ***

